

ANGALABIRI FISH FARM

MATERIALS REQUIRED:

ROAD WORK (400M)

|  |  |  |
| --- | --- | --- |
| S/N | DESCRIPTION | QUANTITY |
| 1 | BACK FILLING OF ROAD, WITH SHARP SAND | 1440M3 |
| 2 | THE NUMBER OF TIPPER TRIPS | 180 TRIPS |
| 3 | B.R.C (WIRE MESH) (4.5-5MM) | 85 ROLLS |
| 4 | AGGREGATE (CHIPPINGS) 12 TRIPS | 360 TONNES |
| 5 | DAMP PROOF MEMBRANE | 32 ROLLS |
| 6 | CEMENT (TWO TRUCKS) | 1800 BAGS |
| 7 | MARINE PLY BOARD | 15 PIECES |
| 8 | NAIL 4m | 4 BAGS |
| 9 | 6MM ROD (QUARTER ROD) | 20 PIECES |

ROOFING OF CONFERENCE HALL

|  |  |  |
| --- | --- | --- |
| S/N | DESCRIPTION | QUANTITY |
| 1 | WALL PLATE 3 x 4 x 12 | 20 LENGTHS |
| 2 | TIE BEAM 2 x 6 x 18 | 50 LENGTHS |
| 3 | RAFTERS 2 x 4 x 18 | 100 LENGTHS |
| 4 | PURLINE AND CEILING NOGGING 2 x 3 x 12 | 150 LENGTHS |

ROOFING SERVICE QHS

|  |  |  |
| --- | --- | --- |
| S/N | DESCRIPTION | QUANTITY |
| 1 | WALL PLATE 3 x 4 x 12 | 36 LENGTHS |
| 2 | TIE BEAM 2 x 6 x 18 | 50 LENGTHS |
| 3 | RAFTERS 2 x 4 x 18 | 200 LENGTHS |
| 4 | PURLINE AND CEILING NOGGING 2 x 3 x 12 | 400 LENGTHS |

RAMP ELEVATION WORK

|  |  |  |
| --- | --- | --- |
| S/N | DESCRIPTION | QUANTITY |
| 1 | 50 TRIPS OF SHARP SAND WITH BOAT/DREDGER | 50 TRIPS |

BACK FILLING OF BUILDINGS OF GENERATOR HOUSE, COLD ROOM/LAB/HATCHERY, SERVICES QRTS, CONFERENCE HALL

|  |  |  |
| --- | --- | --- |
| S/N | DESCRIPTION | QUANTITY |
| 1 | TOTAL VOLUME OF SHARP SAND REQUIRED | 2,472M3 |
| 2 | NUMBER OF TRIPS WITH TIPPERS | 309 TRIPS |

ROOFING SHEET

|  |  |  |
| --- | --- | --- |
| S/N | DESCRIPTION | QUANTITY |
| 1 | GENERATOR HOUSE 120 SQ.M | 135 |
| 2 | WARE HOUSE 450 SQ.M | 500 |
| 3 | COLDROOM/LABORATORY/HATCHERY 550 SQ.M | 600 |
| 4 | SERVICE QUARTER 300 SQ.M | 350 |
| 5 | CONFERENCE HALL 180 SQ.M | 220 |
| 6 | ZINC NAILS |  |
| 7 | GASKET |  |